# SCFG_SetDividerFixed

## Syntax

      #include <twl/scfg.h>

      static inline void SCFG_SetDividerFixed( BOOL sw );

## Arguments

`sw` | If this is `TRUE`, divider circuit revisions will be used. If this is `FALSE`, the circuit will be identical to the NITRO-CPU's.

## Return Values

None.

## Description

Configures the use of revisions to the memory card interface circuit.

If revisions are specified to be used, bugs related to divide-by-zero errors will be fixed.

Revisions will not be used by default.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be invoked on NITRO hardware.

## See Also

SCFG Overview
`SCFG_IsDividerFixed`

## Revision History

2008/04/07 Added information on default values.
2007/10/03 Initial version.

CONFIDENTIAL