# MB_FakeGetParentBssDesc

## Syntax

  `#include <nitro/mb/mb_fake_child.h>`
  `BOOL`
  `MB_FakeGetParentBssDesc( u16 index, WMBssDesc* pBssDesc );`

## Arguments

index | Index for managing the multiboot parent information.
pBssDesc | Pointer to the region for fetching the parent connection information.

## Return Values

`TRUE` if the index argument specifies valid parent information. `FALSE` if the index is not valid.

## Description

This function gets the parent information from the specified index. This information was obtained while scanning for parents. If the specified index is not valid, the function returns FALSE. The information from a valid index can be used to reconnect to the parent after the DS Single-Card Play boot process ends. You can use the `MB_FakeReadParentBssDesc` function to adjust the MP packet size and other settings based on this parent information, and to get information for the `WM_StartConnect` function.
You can also use the `MB_FakeGetParentGameInfo` function to get the parent's game information.

## See Also

`MB_FakeGetParentGameInfo
MB_FakeReadParentBssDesc
WMBssDesc`

## Revision History

2004/11/25 Initial version.

CONFIDENTIAL