# WXC_Stop

## Syntax

  `#include <nitro/wxc.h>`
  `void WXC_Stop(void);`

## Arguments

None.

## Return Values

None.

## Description

Stops wireless operation inside the WXC library.
Calling this function more than once does nothing. By calling this function, the library's internal state transitions from WXC_STATE_ACTIVE to WXC_STATE_READY.
At the point when the transition is actually completed, notification is sent to the callback specified with WXC_Init function.
This function is used to prepare for a restart of chance encounter communication by stopping power supply to wireless started with the WXC_Start function and keeping the LED blinking.
To only end the WXC library, call the WXC_End function directly.

## See Also

`WXCStateCode
WXC_Init
WXC_Start
WXC_End`

## Revision History

2005/10/11 Initial version.

CONFIDENTIAL