MI_ReserveWram

# MI-Related Constants

## Description

###
`MIWramPos` union

Symbol | Description | Comments
--- | --- | ---
`MI_WRAM_A` | Indicates WRAM-A. |
`MI_WRAM_B` | Indicates WRAM-B. |
`MI_WRAM_C` | Indicates WRAM-C. |

### `MIWramProc` union

Symbol | Description | Comments
--- | --- | ---
`MI_WRAM_ARM9` | Indicates ARM9. |
`MI_WRAM_ARM7` | Indicates ARM7. |
`MI_WRAM_DSP` | Indicates DSP. |

### `MIWramEnable` union

Symbol | Description | Comments
--- | --- | ---
`MI_WRAM_ENABLE` | Indicates that [WRAM] is enabled. |
`MI_WRAM_DISABLE` | Indicates that [WRAM] is disabled. |

### `MIWramOffset` union

Symbol | Description | Comments
--- | --- | ---
`MI_WRAM_OFFSET_0KB` | Indicates that the offset is 0 KB. |
`MI_WRAM_OFFSET_32KB` | Indicates that the offset is 32KB. |
`MI_WRAM_OFFSET_64KB` | Indicates that the offset is 64KB. |
`MI_WRAM_OFFSET_96KB` | Indicates that the offset is 96KB. |
`MI_WRAM_OFFSET_128KB` | Indicates that the offset is 128KB. |
`MI_WRAM_OFFSET_160KB` | Indicates that the offset is 160KB. |
`MI_WRAM_OFFSET_192KB` | Indicates that the offset is 192KB. |
`MI_WRAM_OFFSET_224KB` | Indicates that the offset is 224KB. |

###
`MIWramSize` union

Symbol | Description | Comments
--- | --- | ---
`MI_WRAM_SIZE_0KB` | Indicates that the size is 0KB. |
`MI_WRAM_SIZE_32KB` | Indicates that the size is 32KB. |
`MI_WRAM_SIZE_64KB` | Indicates that the size is 64KB. |
`MI_WRAM_SIZE_96KB` | Indicates that the size is 96KB. |
`MI_WRAM_SIZE_128KB` | Indicates that the size is 128KB. |
`MI_WRAM_SIZE_160KB` | Indicates that the size is 160KB. |
`MI_WRAM_SIZE_192KB` | Indicates that the size is 192KB. |
`MI_WRAM_SIZE_224KB` | Indicates that the size is 224KB. |
`MI_WRAM_SIZE_256KB` | Indicates that the size is 256KB. |

###
`MIWramImage` union

Symbol | Description | Comments
--- | --- | ---
`MI_WRAM_IMAGE_32KB` | Indicates that the image region will be repeated in 32-KB units. |
`MI_WRAM_IMAGE_64KB` | Indicates that the image region will be repeated in 64-KB units. |
`MI_WRAM_IMAGE_128KB` | Indicates that the image region will be repeated in 128-KB units. |
`MI_WRAM_IMAGE_256KB` | Indicates that the image region will be repeated in 256-KB units. |

## See Also

Overview (Work RAM)

## Revision History

2007/08/20 Initial version.

CONFIDENTIAL