# CARD_IsBackupFlash

## Syntax

  `#include <nitro/card.h>`
  `static inline BOOL CARD_IsBackupFlash(void);`

## Arguments

None.

## Return Values

Returns TRUE if the designated backup device is FLASH, and FALSE if it is not.

## Description

Determines whether the backup device specified by the `CARD_IdentifyBackup` function is a flash device.

## See Also

`CARD_IdentifyBackup, CARD_ReadFlash, CARD_WriteFlash`

## Revision History

2004/08/23 Revised the links due to changes to the function
2004/08/18 Initial Version

CONFIDENTIAL