# CARD_ProgramAndVerifyFlashAsync

## 構文

  `#include <nitro/card.h>`
  `static inline void CARD_ProgramAndVerifyFlashAsync( u32 dst, const void *src, u32 len, MIDmaCallback callback, void *arg);`

## 引数

dst | 転送先の FLASH アドレス
src | 転送元のメモリアドレス
len | 転送するデータのバイト長
callback | 完了時のコールバック関数 必要ない場合は NULL を指定します。 このコールバックは割り込みハンドラ内から呼び出されます。
arg | 完了時のコールバック関数に与える引数 callback に NULL を指定した場合は単に無視されます。

## 返り値

なし。

## 説明

FLASH デバイスへのデータ書き込み、および書き込んだデータの比較を非同期的に実行します。
この関数はただちに制御を返します。
処理の完了を待つにはCARD_WaitBackupAsync( )を使用します。
処理の結果を判定するには、完了後にCARD_GetResultCode( )を呼び出してください。

この関数で指定する書き込み領域は、前もってCARD_EraseFlashSector( )で内容を消去しておく必要があります。 消去されていない領域に対する書き込みの結果は保証されません。
FLASHデバイスの種類によっては、この関数より制限の少ないCARD_WriteFlash( )が利用可能です。

この関数を使用する場合、事前にアクセスバスをCARD_LockBackup( )でロックしている必要があります。

## 内部動作

`この関数は内部でPXIを介してARM7プロセッサと通信しています。
PXIの割り込みが有効でないと処理が完了しない点に注意してください。
この関数は、内部のスレッドを使用して非同期処理を実行します。
このスレッドに関してはCARD_GetThreadPriority( )の説明を参照ください。
`

## 参照

`CARD_WaitBackupAsync, CARD_GetResultCode, CARD_IsBackupFlash, CARD_ProgramFlash, CARD_ProgramFlashAsync, CARD_ProgramAndVerifyFlash, CARD_ProgramAndVerifyFlashAsync, CARD_EraseFlashSector, CARD_EraseFlashSectorAsync, CARD_WriteFlashSector, CARD_WriteFlashSectorAsync, CARD_WriteAndVerifyFlashSector, CARD_WriteAndVerifyFlashSectorAsync, CARD_ReadFlash, CARD_WriteFlash, CARD_WriteAndVerifyFlash, CARD_VerifyFlash, CARD_GetThreadPriority`

## 履歴

2007/08/22 初版