MI_GetCartridgePriority

# MI_GetCartridgeProcessor

## Syntax

  `#include <nitro/mi.h>`
  `MIProcessor MI_GetCartridgeProcessor( void )`

## Arguments

None.

## Return Values

Settings for access permission to the cartridge.

## Description

This function acquires the permission settings to access AGB compatible 32-pin cartridge slot hardware. The return value is an `MIProcessor` array type that has the following meanings:

`MI_PROCESSOR_ARM9` | Sets access permission to ARM9.
`MI_PROCESSOR_ARM7` | Sets access permission to ARM7.

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`None.
`

## Revision History

2004/10/18 Corrected the return value text.
2004/01/14 Function name changed from `MI_GetCartridgePriority`.
2004/01/14 enum name changed to `MIProcessor`.
2003/12/18 Initial version.

CONFIDENTIAL