# CARD_GetThreadPriority

## Syntax

  `#include <nitro/card.h>`
  `u32 CARD_GetThreadPriority( void );`

## Arguments

None.

## Return Values

Returns the current CARD asynchronous process thread priority.

## Description

Returns the priority of the current CARD asynchronous process thread. This thread is used internally when restrictions on arguments or the operating environment prevent `CARD_ReadRomAsync` and other asynchronous CARD functions from running in an IRQ handler. The priority of this thread is set to `CARD_THREAD_PRIORITY_DEFAULT` by default. It can be changed with the `CARD_SetThreadPriority` function.

## See Also

`CARD_SetThreadPriority
CARD_ReadRomAsync
CARD_ReadEepromAsync
CARD_WriteEepromAsync
CARD_VerifyEepromAsync
CARD_WriteAndVerifyEepromAsync`

## Revision History

2004/07/28 Added descriptions and links.
2004/07/19 Initial Version

CONFIDENTIAL