PAD_Read

# PAD_DetectFold

## Syntax

  `#include <nitro/pad.h>`
  `BOOL PAD_DetectFold( void );`

## Arguments

None.

## Return Values

Returns TRUE when the unit is closed.
Returns FALSE when open.

## Description

Gets whether or not the unit is closed.

Detects the opened/closed state of the unit with the ARM7, and transmits the status to the ARM9.

## Revision History

2004/06/11 Initial version.

CONFIDENTIAL