# VIB_IsExecuting

## Syntax

      #include <nitro/vib.h>

      BOOL VIB_IsExecuting(void);

## Arguments

None.

## Return Values

Returns `TRUE` after pulse vibration is started by the call to the `VIB_StartPulse` function but before pulse vibration is stopped by the call to `VIB_StopPulse`. Otherwise, returns `FALSE`.

## Description

Returns whether pulse vibration is being performed.

After vibrating for the number of times specified in `repeat_num`, it will return `TRUE` until the `VIB_StopPulse` function is called, even if the vibration has stopped.

## Revision History

2008/05/01 Revised the description of the return values.
2005/08/16 Initial version.

CONFIDENTIAL