# TP_GetCalibratedResult

## Syntax

  `#include <nitro/spi.h>`

      u32 TP_GetCalibratedResult( TPData * result );

## Arguments

result | Pointer to the variable to obtain touch-panel values.

## Return Values

0 if touch-panel value is obtained successfully.
Non-zero value if task fails due to some error.

## Description

Considers the touch-panel values requested by the `TP_RequestSamplingAsync` function to have been set by the ARM7, and gets these values as calibrated screen coordinates. (X value ranges between 0 and 255; Y value ranges between 0 and 191) The value obtained here already accounts for chattering. If a response from ARM7 has not come yet, it may not be possible to obtain a correct value.

## See Also

`TP_RequestSamplingAsync`, `TP_WaitCalibratedResult`, `TP_WaitRawResult`, `TPData`

## Revision History

2004/04/16 Initial version.

CONFIDENTIAL