WVR Demos

# Wireless Driver Operation Control Library (WVR) Sample Demos

## Location

`$TwlSDK/build/demos/wvr`

## Compilation

Move to the `$TwlSDK/build/demos/wvr` directory and enter the following.

> `% make`

The compilation begins, and the SRL executable file and the NEF files with binary information are generated in the following directory.

> `$TwlSDK/build/demos/wvr/sample_name/bin/platform/target/`

For example:

> `$TwlSDK/build/demos/wvr/simple/bin/ARM9-TS/Release/main.srl`

The above path shows the executable file for the `simple` demo.

## Execution

### For NITRO ROMs

If using IS-NITRO-DEBUGGER:

- Load and execute an NLF file with IS-NITRO-DEBUGGER
- Execute an SRL file with IS-NITRO-DEBUGGER
- Execute an SRL file with IS-NITRO-DEBUGGER using the `loadrun.exe` tool from the command line

If using IS-TWL-DEBUGGER:

- Load and execute an NLF file with IS-TWL-DEBUGGER
- Execute an SRL file with IS-TWL-DEBUGGER
- Execute an SRL file with IS-TWL-DEBUGGER using the `loadrun.TWL.exe` tool from the command line

## Description

Name | Directory | Operation
--- | --- | ---
`simple` | `demos` | A simple sample that demonstrates communications using VRAM-D in wireless communications through the WVR library.
`switchover` | `demos` | A sample that switches allocations for single VRAMs to rendering use or communications use. Display of the following sample demos is toggled by pressing the Select button. `/build/demos/wvr/simple` `/build/demos/gx/UnitTours/Sub_Double3D`
`with_mb` | `demos` | A sample used when the WVR library is in DS download play. It is based on the following sample: `/build/demos/mb/multiboot-Model`

## Operation

``The WVR library demos work properly only with NITRO ROMs.

## See Also

`WVR Function List`

## Revision History

2009/08/31 Changed button for selecting switchover.
2008/07/11 Changed the description to match TWL.
2005/02/17 Initial version.

CONFIDENTIAL