# SCFG_SupplyClockToDSP

## Syntax

      #include <twl/scfg.h>

      static inline void SCFG_SupplyClockToDSP( BOOL sw );

## Arguments

sw | If `TRUE`, a clock will be supplied to the DSP block. If `FALSE`, a clock will no longer be supplied.

## Return Values

None.

## Description

Configures the clock supply to the DSP block.

To be safe, stop the clock while the DSP block is stopped.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be called on NITRO hardware.

## See Also

SCFG Overview
`SCFG_IsClockSuppliedToDSP`

## Revision History

2007/10/03 Initial version.

CONFIDENTIAL