CTRDG Demos

# Rumble Pak Sample Demo

## Location

`$TwlSDK/build/demos/vib`

## Compilation

Move to the `$TwlSDK/build/demos/vib` directory and enter the following:

> `% make`

Compiling will begin, and the SRL executable file and the NEF or TEF files having binary information will be generated in `$TwlSDK/build/demos/vib/(sample name)/bin/(platform)/(target)/`.

For example:

> `$TwlSDK/build/demos/vib/pulse_vib/bin/ARM9-TS/Release/main.srl`

will be the executable file for the `pulse_vib` demo.

## Execution

### For NITRO ROMs

If using IS-NITRO-DEBUGGER:

- Load and execute an NLF file with IS-NITRO-DEBUGGER
- Execute an SRL file with IS-NITRO-DEBUGGER
- Execute an SRL file with IS-NITRO-DEBUGGER using the `loadrun.exe` tool from a command line

### For TWL/NITRO Hybrid ROMs

If using IS-NITRO-DEBUGGER:

- Execute an SRL file with IS-NITRO-DEBUGGER
- Execute an SRL file with IS-NITRO-DEBUGGER using the `loadrun.exe` tool from a command line

## Description

Name | Directory | Operation
--- | --- | ---
`pulse_vib` | `demos` | Sample that allows any pulse to be generated for the Rumble Pak.

## Operation

The `pulse_vib` demo works properly only with the IS-NITRO-DEBUGGER.

## See Also

VIB Function List

## Revision History

2008/07/11 Changed descriptions to support TWL.
2006/03/02 Initial version.

CONFIDENTIAL