# DSP_GetLastSamplingAddress

## Syntax

    const u8* DSP_GetLastSamplingAddress(void);

## Arguments

None.

## Return Values

Ring buffer address storing the most recent sampling data. This address will use the buffer specified by the `DSP_StartSampling` function as a ring buffer by wrapping around it within the size range.

## Description

Gets the most recent position as a ring buffer address to which data was saved during automatic sampling started by the `DSP_StartSampling` function. This sampling position will be updated each time the `DSP_SyncSamplingBuffer` function is called.

## See Also

`DSP_StartSampling DSP_StopSampling DSP_SyncSamplingBuffer`

## Revision History

2008/06/13 Initial version.

CONFIDENTIAL