# CARDBackupType

## 定義

  `#include <nitro/card.h>`
  `typedef enum {
  CARD_BACKUP_TYPE_EEPROM_4KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 9, 0),
  CARD_BACKUP_TYPE_EEPROM_64KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 13, 0),
  CARD_BACKUP_TYPE_EEPROM_512KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 16, 0),
  CARD_BACKUP_TYPE_EEPROM_1MBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 17, 0),
  CARD_BACKUP_TYPE_FLASH_2MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 18, 0),
  CARD_BACKUP_TYPE_FLASH_4MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 19, 0),
  CARD_BACKUP_TYPE_FLASH_8MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 20, 0),
  CARD_BACKUP_TYPE_FLASH_16MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 21, 0),
  CARD_BACKUP_TYPE_FLASH_64MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 23, 0),
  CARD_BACKUP_TYPE_NOT_USE = 0
  } CARDBackupType;`

## 説明

NITRO-CARD に搭載されるバックアップデバイスを識別する列挙定数を示します。

## 参照

`CARD_IdentifyBackup, CARD_GetCurrentBackupType`

## 履歴

2008/11/27 採用可能なラインナップからCARD_BACKUP_TYPE_FRAM_256KBITSを削除
2008/10/21 CARD_BACKUP_TYPE_EEPROM_1MBITSを追加
2007/08/22 CARD_BACKUP_TYPE_FLASH_64MBITSを追加
2007/02/23 CARD_BACKUP_TYPE_FLASH_16MBITSを追加
2006/04/05 CARD_BACKUP_TYPE_FLASH_8MBITSを追加
2005/10/19 CARD_BACKUP_TYPE_FLASH_4MBITSを追加
2005/07/11 CARD_BACKUP_TYPE_FRAM_256KBITSを追加
2005/06/15 CARD_BACKUP_TYPE_EEPROM_512KBITSを追加
2004/09/09 CARD_BACKUP_TYPE_EEPROM_512KBITS, CARD_BACKUP_TYPE_EEPROM_1MBITSを削除
2004/08/23 列挙値の形式を変更、CARD_BACKUP_TYPE_FLASH_2MBITSを追加
2004/07/05 初版