# NNS_G3D_SBC_RET

## Command Format

Offset (bytes) | Description
--- | ---
0 | `NNS_G3D_SBC_RET`

## Description

The `NNS_G3D_SBC_RET` command ends the SBC processing by setting the `NNS_G3D_RSFLAG_RETURN` bit of the flag contained in the `NNS_G3dRS` structure. A callback process can be inserted only once, and regardless of which kind of timing is designated, the callback function is executed in the same general location. This is a 1-byte command and does not have an operand.

Timing for Calling a Callback Function | Usage
--- | ---
`NNS_G3D_SBC_CALLBACK_TIMING_A` | The callback function will be called at the same place regardless of the timing that is specified.
`NNS_G3D_SBC_CALLBACK_TIMING_B`
`NNS_G3D_SBC_CALLBACK_TIMING_C`

## See Also

## Revision History

2004/10/14 Added description.
2004/08/02 Initial version.

CONFIDENTIAL