# NNS_G2dSetCellTransferStateRequested

## Syntax

      #include <nnsys/g2d/g2d_CellTransferManager.h>

      void NNS_G2dSetCellTransferStateRequested(
                                  u32     handle,
                                  u32     srcOffset,
                                  u32     szByte );

## Arguments

`handle` | [IN] Handle of cell VRAM transfer state object
`srcOffset` | [IN] Offset value from the start of the transfer source data
`szByte` | [IN] Transfer size

## Return Values

None.

## Description

Sets the cell VRAM transfer state object in the VRAM transfer request state. For the state object set in the VRAM transfer request state, a VRAM transfer is actually requested if the `NNS_G2dUpdateCellTransferStateManager` function is checked and the "to be drawn" flag is valid.

## See Also

`NNS_G2dUpdateCellTransferStateManager`

## Revision History

2004/07/20 Initial version.

CONFIDENTIAL