# NNS_G2dEntryNewOamEx

## Syntax

      #include <nnsys/g2d/g2d_OAMEx.h>

      BOOL NNS_G2dEntryNewOamEx(
                                  NNSG2dOamManagerInstanceEx*     pMan,
                                  const GXOamAttr*                pOam,
                                  u8                              priority );

## Arguments

`pMan` | [OUT] Extended OAM manager entity
`pOam` | [IN] OAM attribute
`priority` | [IN] Display priority (order of registration when rendering)

## Return Values

Success or failure of registration.

## Description

Specifies the order of registration of OBJs in the extended OAM Manager when rendering, and registers the OBJs. When actually applied to the hardware, this function registers OBJs to the OAM in the designated display priority order.
The name of this function has changed to `NNS_G2dEntryOamManExOam`. This function will remain with a separate name to maintain compatibility.

## See Also

`NNS_G2dEntryOamManExOam`
`NNS_G2dEntryOamManExOamWithAffineIdx`

## Revision History

2004/08/02 Renamed function.
2004/06/22 Initial version.

CONFIDENTIAL