# NNS_G2dApplyToHW

## Syntax

      #include <nnsys/g2d/g2d_Oam.h>

      void NNS_G2dApplyToHW(
              NNSG2dOamManagerInstance*   pMan );

## Arguments

`pMan` | [IN] OAM manager entity.

## Return Values

None.

## Description

Reflects the internal state of the OAM manager to the actual hardware. This function must be called during a V-blank event if the manager type is not `NNS_G2D_OAMTYPE_SOFTWAREEMULATION`. If the manager type is `NNS_G2D_OAMTYPE_SOFTWAREEMULATION`, this function can be called even if it is not during a V-blank event. The name of this function has changed to `NNS_G2dApplyOamManagerToHW`. To maintain compatibility with past versions, this function has been kept under a different name.

## See Also

`NNS_G2dApplyOamManagerToHW`
`NNS_G2dResetOamManagerBuffer`

## Revision History

2004/08/02 Renamed function.

2004/05/28 Initial version.

CONFIDENTIAL