# Viewing LLDP protocol properties

Use this procedure to view LLDP protocol properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click Port dot1.

5. Select the Local Protocol tab.

The following table outlines the parameters of the Local Protocol tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
ProtocolIndex | Specifies an arbitrary local integer value used by this agent to identify a particular protocol identity.
ProtocolId | Specifies the octet string value used to identify the protocols associated with the given port of the local system.
ProtocolTxEnable | Indicates whether the corresponding Local System Protocol Identity instance is transmitted on the port.

Parent topic: LLDP Port dot1 configuration using Enterprise Device Manager