# Viewing Priority Q Assign

Use this procedure to open the Priority Q Assign tab.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS Devices.

3. Select the Priority Q Assign tab.

## Variable definitions

The following table outlines the parameters of the Priority Q Assign tab.

Table 1. QoS Devices Priority Q Assign tab parameters
Variable | Value
--- | ---
Qset | Represents the queue set number. Supports the assignment of 802.1p user priority values to a queue for each specific queue set. There are 56 instances for queue set number, each instance is a multiple of one basic queue-set from 1 to 8.
802.1pPriority | A 802.1 user priority value.
Queue | A queue in a specified queue set that is assigned a priority value. To change a Queue assignment, click in the cell and type a new value.