# Viewing LLDP maximum frame size properties

Use this procedure to view LLDP maximum frame size properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Local Max Frame tab.

The following table outlines the parameters of the Port dot3 Local Max Frame tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number
MaxFrameSize | Specifies the maximum frame size for the port

Parent topic: LLDP Port dot3 configuration using Enterprise Device Manager