# Displaying boot image and flash information

Use the following procedure to display the currently loaded and operational agent, image, and flash load status for the switch or stack.

## Procedure

1. From the navigation tree, double-click Edit.
2. In the Edit tree, click File System.
3. In the work area, click the FLASH tab.

## Variable definitions

The following table describes displaying boot images.

Variable | Value
--- | ---
Unit | Specifies the unit.
Type | Specifies the type of image.
Version | Specifies the software version of the image.
Description | Specifies a description of the image.
Age | Specifies the age.