# Filtering route information

Use the following procedure to filter the Routes tab to display only the desired switch routes.

## Procedure steps

1. From the navigation tree, double-click IP Routing.

2. In the IP Routing tree, double-click IP.

3. In the work area, select the Routes tab.

4. In the toolbar, click Filter.

## Variable definitions

The following table describes the fields of the Filter tab.

Field | Description
--- | ---
Condition | When you use multiple filter expressions on the tab, the condition joins them together.
Ignore Case | Denotes whether filters are case sensitive or insensitive.
Column | Denotes the type of criteria that will apply to values for filtering.
All Records | Clears the filters, and displays all rows.
Dest | Select this check box and enter a value to filter on the route destination value.
Mask | Select this check box and enter a value to filter on the route destination subnet mask value.
NextHop | Select this check box and enter a value to filter on the next hop value of the route.
HopOrMetric | Select this check box and enter a value to filter on the hop count or metric of the route.
Interface | Select this check box and enter a value to filter on the associated interface of the route.
Proto | Select this check box and enter a value to filter on the route protocol.
PathType | Select this check box and enter a value to filter on the route path type.
Pref | Select this check box and enter a value to filter on the route preference value.