# Viewing DHCP binding information using EDM

Use the following procedure to display DHCP binding information.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security Routing tree, double-click DHCP Snooping.

3. In the work area, click the DHCP Bindings tab.

## Variable definitions

Use the data in the following table to help you understand the DHCP binding information display.

Variable | Value
--- | ---
VlanId | Indicates the ID of the VLAN that the DHCP client is a member of.
MacAddress | Indicates the MAC address of the DHCP client.
AddressType | Indicates the MAC address type of the DHCP client.
Address | Indicates IP address of the DHCP client.
Interface | Indicates the interface to which the DHCP client is connected.
LeaseTime(sec) | Indicates the lease time (in seconds) of the DHCP client binding. Values range from 0 to 4294967295.
TimeToExpiry(sec) | Indicates the time (in seconds) before a DHCP client binding expires.
Source | Indicates the source of the binding table entry