# Viewing LLDP organizationally-specific properties

Use this procedure to view Organizationally-specific properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click LLDP.

5. Select the Organizational Defined Info tab.

The following table outlines the parameters of the Organizational Defined Info tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Specifies an arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
OrgDefInfoOUI | Specifies the Organizationally Unique Identifier (OUI), as defined in IEEE 802-2001, is a 24 bit (three octets) globally unique assigned number referenced by various standards, of the information received from the remote system.
OrgDefInfoSubtype | Identifies the subtype of the organizationally defined information received from the remote system. The subtype value is required to identify different instances of organizationally defined information that cannot be retrieved without a unique identifier that indicates the particular type of information contained in the information string.
OrgDefInfoIndex | Represents an arbitrary local integer value used by this agent to identify a particular unrecognized organizationally defined information instance, unique only for the OrgDefInfoOUI and lldpRemOrgDefInfoSubtype of the same remote system. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot. It is unlikely that the lldpRemOrgDefInfoIndex will wrap between reboots.
OrdDefInfo | Identifies the organizationally defined information of the remote system. The encoding for this object is the same as that defined for SnmpAdminString TC.

Parent topic: LLDP configuration using Enterprise Device Manager