# Creating a new MIB view using EDM

Use the following procedure to create a new MIB view.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Snmp Server.

3. In the Snmp Server tree, double-click MIB View.

4. In the toolbar, click Insert.

   The Insert MIB View dialog box appears.

5. Configure the parameters as required.

6. Click Insert.

## Variable definitions

The following table describes the fields of MIB View tab.

Variable | Value
--- | ---
ViewName | Specifies a new entry with this group name. The range is 1 to 32 characters.
Subtree | Specifies a valid object identifier that defines the set of MIB objects accessible by this SNMP entity, for example, 1.3.6.1.1.5
Type | Determines whether access to a mib object is granted (Included) or denied (Excluded). Included is the default.
StorageType | Indicates the storage type for the view.

## Deleting an MIB view using EDM

Use the following procedure to delete an MIB view.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Snmp Server.

3. In the Snmp Server tree, double-click MIB View.

4. In the work area, select the record that you want to delete.

5. In the toolbar, click Delete.