# Configuring MAC Address AutoLearn using EDM

Use the following procedure to configure the MAC Address auto learning properties of switch ports.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click MAC Security.

3. In the work area, click the AuthLearn tab.

4. In the table, double-click the cell under the column heading for the parameter that you want to change.

5. Select a parameter or value from the drop-down list.

6. Repeat the previous two steps until you have amended all of the parameters that you want to change.

7. In the toolbar, click Apply.

## Variable definitions

Use the data in the following table to configure MAC Address AutoLearn.

Variable | Value
--- | ---
Unit | Identifies the board.
Port | Identifies the port.
Enabled | Enables or disables AutoLearning on a port. Values are true or false.
MaxMacs | Defines the maximum number of MAC Addresses that the port can learn.