# Configuring RIP in and out policies

Use the following procedure to configure RIP accept and announce policies.

## Procedure steps

1. From the navigation tree, double-click IP.

2. In the IP tree, click Policy.

3. In the work area, click the Route In/Out Policy tab.

4. In the table, double-click the cell under the column heading for the parameter you want to change.

5. Select a parameter or value from the drop-down list.

6. Repeat the previous two steps until you have amended all of the parameters you want to change.

7. In the toolbar, click Apply.

## Variable definitions

The following table describes the fields of the RIP In/Out Policy tab.

Field | Definition
--- | ---
Address | Specifies the address of the RIP interface.
Interface | Specifies the associated switch interface.
InPolicy | Specifies a previously configured policy to be used as the accept policy on this interface.
OutPolicy | Specifies a previously configured policy to be used as the announce policy on this interface.