# Downloading a binary configuration file from a TFTP server using EDM

## About this task

Use this procedure to download a binary configuration file from a TFTP server.

## Procedure

1. From the Navigation tree, double-click Edit.
2. From the Edit tree, double-click File System.
3. Select the Config/Image/Diag File tab.
4. In TftpServerInetAddress, enter the TFTP server IP address.
5. In BinaryConfigFilename, enter the configuration file name.
6. In Action, click dnldConfig.
7. On the toolbar, click Apply.