# Viewing LLDP VLAN ID properties

With the Local VLAN Id tab, you can view LLDP VLAN ID properties for the local system.

To open the Local VLAN Id tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot1.

5. Select the Local VLAN Id tab.

The following table outlines the parameters of the Port dot1 Local VLAN Id tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Port number.
VlanId | The local port VLAN ID. A value of zero is used if the system does not know the PVID.