# Viewing RADIUS Dynamic Server statistics using EDM

Use the following procedure to display and review RADIUS Dynamic Server statistical information.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click 802.1X/EAP.

3. In the work area, click the RADIUS Dynamic Server Stats tab.

## Variable definitions

Use the data in the following table to view RADIUS Dynamic Server statistics.

Variable | Value
--- | ---
ClientIndex | Indicates the RADIUS Dymanic Server client index.
ClientAddressType | Indicates the type of RADIUS Dymanic Server address. Values are ipv4 or ipv6.
ClientAddress | Indicates the IP address of the RADIUS Dymanic Server.
ServerCounterDiscontinuity | Indicates a count of RADIUS Dymanic Server discontinuity instances.