# Viewing LLDP neighbor maximum frame size properties

With the Neighbor Max Frame tab, you can view LLDP maximum frame size properties for the remote system.

To view the Neighbor Max Frame tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Neighbor Max Frame tab.

The following table outlines the parameters of the Port dot3 Neighbor Max Frame tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | The TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | An arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
MaxFrameSize | Maximum Frame Size for the remote port.