# Disabling MLT ports on Shutdown

Use this procedure to configure the system to disable MLT ports on shutdown.

1. From the navigation tree, click VLAN.

2. From the VLAN tree, click MLT/LACP.

3. Select the Globals tab.

4. Select the MltDisablePortsOnShutdown check box.

5. In the SmltSysId field, enter the LACP system ID for SMLT (MAC address).

6. On the tool bar, click Apply.

Table 1. Variable definitions
Variable | Value
--- | ---
MltDisablePortsOnShutdown | Specifies whether the function is enabled or disabled.
SmltSysId | Specifies the MAC address of the LACP system ID for SMLT.