# Viewing LLDP auto-negotiation properties

With the Local Port Auto-negotiation tab, you can view LLDP auto-negotiation properties for the local system.

To view the Local Port Auto-negotiation tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Local Port Auto-negotiation tab.

The following table outlines the parameters of the Port dot3 Local Port Auto-negotiation tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Port number.
AutoNegSupported | Indicates whether the local port supports Auto-negotiation.
AutoNegEnabled | Indicates whether Auto-negotiation is enabled on the local port.
AutoNegAdvertisedCap | This object contains the value (bitmap) of the ifMauAutoNegCapAdvertisedBits object (defined in IETF RFC 3636) associated with the local port on the system.
OperMauType | A value that indicates the operational MAU type of the given port on the local system.