# Viewing actions

Use this procedure to open the action tab.

This section discusses the management and use of QoS actions, interface action extensions, meters, and policies.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS.

3. Select the Action tab.

## Variable definitions

The following table outlines the parameters of the Action tab.

Table 1. QoS Action tab parameters
Variable | Value
--- | ---
Id | Specifies the identifier for the action.
Name | Specifies a name for the action.
Drop | Specifies whether a packet is dropped, not dropped, or whether the decision is deferred.
UpdateDscp | Specifies a value used to update the DSCP field in an IPv4 packet.
SetDropPrecedence | Specifies automatic drop precedence.
UpdateUserPriority | Specifies a value for the 802.1p user priority.
Extension | Specifies linking additional actions. (These are defined on the Interface Action Ext Table.)
SessionId | Specifies the numerical identification for the active session.
Storage | Specifies the type of storage: volatile nonVolatile readOnly

This section contains information about the following topics:

- Adding QoS actions

- Deleting QoS actions