# Viewing LLDP maximum frame size properties

With the Local Max Frame tab, you can view LLDP maximum frame size properties for the local system.

To view the Local Max Frame tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot3.

5. Select the Local Max Frame tab.

The following table outlines the parameters of the Port dot3 Local Max Frame tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | port number
MaxFrameSize | maximum frame size for the port