# Viewing LLDP protocol properties

With the Local Protocol tab, you can view LLDP protocol properties for the local system.

To open the Local Protocol tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot1.

5. Select the Local Protocol tab.

The following table outlines the parameters of the Port dot1 Local Protocol tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Port number.
ProtocolIndex | An arbitrary local integer value used by this agent to identify a particular protocol identity.
ProtocolId | The octet string value used to identify the protocols associated with the given port of the local system.
ProtocolTxEnable | Indicates whether the corresponding Local System Protocol Identity instance is transmitted on the port.