# Configuring remote access

Use the following procedure to configure remote access for a switch or stack.

## Procedure

1. From the navigation tree, double-click Administration.
2. In the Administration tree, click Remote Access.
3. In the work area, click the Setting tab.
4. In the Telnet Access Setting section, select a value from the Access list.
5. In the Telnet Access Setting section, select a value from the Use List list.
6. In the SNMP Remote Access Setting section, select a value from the Access list.
7. In the SNMP Remote Access Setting section, select a value from the Use List list.
8. In the Web Page Remote Access Setting section, select a value from the Use List list.
9. In the SSH Remote Access Setting section, select a value from the Access list.
   Note

   SSH Remote Access is only available in secure software builds.

10. In the SSH Remote Access Setting section, select a value from the Use List list.
    Note

    SSH Remote Access is only available in secure software builds.

11. On the toolbar, click Apply.

## Variable Definitions

The data in the following table describes configuring remote access for a switch or stack using EDM.

Variable | Value
--- | ---
Telnet Remote Access Setting | Specifies the remote access settings for telnet sessions. If you need to describe a series of choices for the field, use an unordered list as follows: Access: allows or denies telnet access to the switch or stack. Use List: Enables (Yes) or disables (No) the use of remote access list Telnet information.
SNMP Remote Access Setting | Specifies the remote access settings for SNMP. If you need to describe a series of choices for the field, use an unordered list as follows: Access: allows or denies SNMP access to the switch or stack. Use List: Enables (Yes) or disables (No) the use of remote access list SNMP information.
Web Page Remote Access Setting | Specifies the remote access settings for Web Page. If you need to describe a series of choices for the field, use an unordered list as follows: Use List: Enables (Yes) or disables (No) the use of remote access list web page information.
SSH Remote Access Setting | Specifies the remote access settings for SSH. Note SSH is only available in secure software builds. If you need to describe a series of choices for the field, use an unordered list as follows: Access: allows or denies SSH access to the switch or stack. Use List: Enables (Yes) or disables (No) the use of remote access list SSH information.