# Configuring a VRF instance

Use this procedure to modify the configuration parameters for an existing VRF instancel

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click VRF.

3. In the VRF work area, double-click an Id cell, to modify the configuration for that parameter.

4. On the toolbar, click Apply.

5. On the toolbar, you can click Refresh to verify the VRF instance configuration.

## Variable definitions

Variable | Value
--- | ---
Id | Specifies a numerical ID for the VRF instance. Values range from 1 to 3.
Name | Specifies the alphanumeric identifier (name) assigned to the VRF instance.
MaxRoutes | Specifies a maximum number of routes for the VRF instance. Values range from 0 to 500.