# Viewing Multihost DHCP Authenticated information

Use this procedure to view multiple host DHCP authenticated information for a port.

Important

The Multi Hosts and Non-EAP MAC buttons are not available when configuring multiple ports on the EAPOL Advance tab. To make use of these two options, you can select only one port.

## Procedure steps

1. In the Device Physical View, select a port.

2. Right-click the selected Port.

3. In the shortcut menu, click Edit.

4. In the work area, click the EAPOL Advance tab.

5. In the toolbar, click Multi Host.

6. In the work area, click the Multi Host DHCP Authenticated tab to view multi host DHCP authentication information.