# Viewing LLDP remote management properties

With the Neighbor Mgmt Address tab, you can view LLDP management properties for the remote system.

To open the Neighbor Mgmt Address tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click LLDP.

5. Select the Neighbor Mgmt Address tab.

The following table outlines the parameters of the LLDP Neighbor Mgmt Address tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | The TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | An arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
AddrSubtype | The type of encoding used in the associated Addr object.
Addr | The management address associated with the remote system.
AddrIfSubtype | Identifies the numbering method used to define the interface number associated with the remote system. unknown ifIndex systemPortNumber
AddrIfId | The integer value used to identify the interface number of the management address component associated with the remote system.
AddrOID | The value used to identify the type of hardware component or protocol entity associated with the management address advertised by the remote system agent.