# Viewing the resource allocation configuration for ERS 5500

Use this procedure to view the resource allocation configuration for the ERS 5500 switch.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS Agent.

3. Select the Resource Allocation (ERS5500) tab.

## Variable definitions

Variable | Value
--- | ---
Port | Displays the port number.
MasksConsumed | Displays the number of QoS masks (policies) in use on that interface.
FiltersConsumed | Displays the number of rules (filters) in use by policy and filter data by that interface.
MetersConsumed | Displays the number of meters in use by policy data by that interface.
CountersConsumed | Displays the number of counters in use by that interface.
NonQosMasksConsumed | Displays the number of Non QoS masks (policies) in use on that interface.
NonQosFiltersConsumed | Displays the number of rules (filters) in use by Non QoS policy and filter data by that interface.
NonQosMetersConsumed | Displays the number of meters in use by Non QoS policy data by that interface.