# Storing a binary configuration file on a TFTP server using EDM

## About this task

Use this procedure to store a binary configuration file on a TFTP server.

## Procedure

1. From the Navigation tree, double-click Edit.
2. From the Edit tree, double-click File System.
3. Select the Config/Image/Diag File tab.
4. In TftpServerInetAddress, enter the TFTP server IP address.
5. In BinaryConfigFilename, enter the configuration file name.
6. In Action, click upldConfig.
7. On the toolbar, click Apply.