# Deleting a MAC address from the allowed non-EAP MAC address list using EDM

Use the following procedure to delete a MAC address from the allowed non-EAP MAC address list.

## Procedure steps

1. In the Device Physical View, select a port.

2. Right-click the selected Port.

3. In the shortcut menu, click Edit.

   The Port tab appears.

4. In the work area, click the EAPOL Advance tab.

5. In the toolbar, click Non-EAP MACHost.

   The Non-EAP MAC, Port tab appears with Allowed non-EAP MAC tab opened.

6. In the work area, select the MAC address you want to delete.

7. In the toolbar, click Delete.

8. Click Yes to confirm.