# Viewing unit statistics using EDM

Use the following procedure to view the statistical information of a unit.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

1. In the Device Physical View, select the unit.

2. From the navigation tree, double-click Edit.

3. In the Edit tree, double-click Unit.

4. In the work area, click the Unit Stats tab to view the statistical information of the selected unit.

## Variable definitions

The following table describes the fields of Unit Stats tab.

Field | Description
--- | ---
Absolute Value | Indicates the counter value of packets dropped for the unit.
Cumulative | Indicates the total value of packets dropped seen since dialog displayed.
Average/sec | Indicates the average value of packets dropped per second.
Minimum/sec | Indicates the smallest value of packets dropped seen per second.
Maximum/sec | Indicates the largest value of packets dropped seen per second.
LastVal/sec | Indicates the last value of packets dropped seen per second.