# Configuring interface queue shaper

The following sections describe the Interface queue shaper.

## Viewing QoS interface queue shaper information

Use this procedure to view QoS interface queue shaper information.

### Procedure steps

1. From the navigation tree, double-click QoS.

2. In the QoS tree, double-click QoS .

3. In the work area, click the Interface Queue Shaper tab.

Variable definitions

Use the data in the following table to help you understand QoS interface queue shaper information.

Table 1. Interface Queue Shaper parameters
Variable | Value
--- | ---
Port | Indicates the interface port number associated with a QoS interface shaper. The port number must correspond to the interface table entry with the same port number.
Queue | Indicates the queue for the selected interface port or ports, on which traffic is shaped. The range of available values is determined by the OoS agent default queue configuration.
Name | Indicates an alphanumeric label used to identify the QoS interface queue shaper.
ShapingRate | Indicates the QoS interface queue shaping rate, in kilobits per second (Kbps). Values range from 0 to10230000 Kbps. The values must be a multiple of 64 or 1000 Kbps.
ShapingMinRate | Indicates the minimum QoS interface queue shaping rate, in kilobits per second (Kbps). Values range from 0 to10230000 Kbps. The value must be a multiple of 64 or 1000 Kbps.

## Creating a QoS interface queue shaper

Use this procedure to create a new QoS interface queue shaper.

### Procedure steps

1. From the navigation tree, double-click QoS.

2. In the QoS tree, double-click QoS.

3. In the work area, click the Interface Queue Shaper tab.

4. Click Insert.

5. Click the Ports ellipsis.

6. Click the required ports for the interface queue.

7. Click Ok.

8. In the Queue box, type a value.

9. In the Name box, type a character string.

10. In the ShapingRate box, type a value.

11. In the ShapingMinRate box, type a value.

12. Click Insert.

Variable Definitions

Use the data in the following table to help you create a new QoS interface queue shaper.

Table 2. Interface Queue Shaper parameters
Variable | Value
--- | ---
Port | Specifies the interface port number associated with a QoS interface shaper. The port number must correspond to the interface table entry with the same port number.
Queue | Specifies the queue for the selected interface port or ports, on which traffic is shaped. The range of available values is determined by the OoS agent default queue configuration.
Name | Specifies an alphanumeric label used to identify the QoS interface queue shaper.
ShapingRate | Specifies the QoS interface queue shaping rate, in kilobits per second (Kbps). Values range from 64 to 10230000 Kbps. The value must be a multiple of 64 or 1000 Kbps.
ShapingMinRate | Specifies the minimum QoS interface queue shaping rate, in kilobits per second (Kbps). Values range from 0 to 10230000 Kbps. The value must be a multiple of 64 or 1000 Kbps.

## Deleting a QoS interface queue shaper

Use this procedure to delete a QoS interface shaper.

### Procedure steps

1. From the navigation tree, double-click QoS.

2. In the QoS tree, double-click QoS.

3. In the work area, click the Interface Queue Shaper tab.

4. To select a queue shaper to delete, click the queue shaper row.

5. On the toolbar, click Delete.