# Viewing LLDP local port properties

Use this procedure to view LLDP port properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click LLDP.

5. Select the Local System tab.

The following table outlines the parameters of the Local Port tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
PortIdSubtype | Specifies the type of port identifier encoding used in the associated PortId object. interfaceAlias portComponent macAddress networkAddress interfaceName agentCircuitId local.
PortId | Iidentifies the port component associated with a given port in the local system.
PortDesc | Identifies the 802 LAN station port description associated with the local system. If the local agent supports IETF RFC 2863, the PortDesc object has the same value as the ifDescr object.