# Viewing LLDP VLAN ID properties

Use this procedure to view LLDP VLAN ID properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click Port dot1.

5. Select the Local VLAN Id tab.

The following table outlines the parameters of the Local VLAN Id tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
VlanId | Specifies the local port VLAN ID. A value of zero is used if the system does not know the PVID.